Power supply

7600W continuous with 2X peak and able to rectify 208VAC

L60-300VDC gets full torque at around 200VDC

Weight of the current servo/gearbox = 8lbs

Reduction ratio using the elmo servo ~7-10

Gearbox weight reduction using wittenstein 52lbs

Possible options